



**NP112-IR/25X**

**2MP 25× Network IR Speed Dome**



|  |  |
| --- | --- |
| NP112-IR/25X 2MP 25× Network IR Speed Dome adopts 1/2.8" progressive scan CMOS chip. With the 25× optical zoom lens, the camera offers more details over expansive areas.  This series of cameras can be widely used for wide ranges of high-definition, such as the rivers, roads, railways, airports, squares, parks, scenic spots, and venues, etc. | **Key Features**   * 1/2.8" progressive scan CMOS * Up to 1920 × 1080@30fps resolution * Min. illumination:   Color: 0.005 Lux @(F1.6, AGC ON)  B/W: 0.001 Lux @(F1.6, AGC ON)  0 Lux with IR   * 25× optical zoom, 16× digital zoom * WDR, HLC, BLC, 3D DNR, Defog, EIS, Regional Exposure, Regional Focus * Up to 100 m IR distance * 12 VDC & PoE+ (802.3 at, class4) * Support H.265+/H.265 video compression |

**Specification**

|  |  |
| --- | --- |
| **Camera Module** | |
| Image Sensor | 1/2.8" progressive scan CMOS |
| Min. Illumination | Color: 0.005 Lux @(F1.6, AGC ON)  B/W: 0.001Lux @(F1.6, AGC ON)  0 Lux with IR |
| White Balance | Auto/Manual/ATW (Auto-tracking White Balance)/Indoor/Outdoor/Fluorescent Lamp/Sodium Lamp |
| Gain | Auto/Manual |
| Shutter Time | 50Hz: 1/1 s to 1/30,000 s  60Hz: 1/1 s to 1/30,000 s |
| Day & Night | IR Cut Filter |
| Digital Zoom | 16× |
| Privacy Mask | 24 programmable privacy masks |
| Focus Mode | Auto/Semi-automatic/Manual |
| WDR | 120 dB WDR |
| **Lens** | |
| Focal Length | 4.8 mm to 120 mm, 25× optical zoom |
| Zoom Speed | Approx. 3.6 s (optical lens, wide-tele) |
| Field of View | Horizontal field of view: 57.6° to 2.5° (Wide-Tele)  Vertical field of view: 34.4° to 1.4° (Wide-Tele)  Diagonal field of view: 64.5° to 2.9° (Wide-Tele) |
| Working Distance | 10 mm to 1500 mm (wide-tele) |
| Aperture Range | F1.6 to F3.5 |
| **IR** | |
| IR Distance | 100 m |
| Smart IR | Support |
| **PTZ** | |
| Movement Range (Pan) | 360° endless |
| Pan Speed | Configurable, from 0.1°/s to 80°/s,  Preset speed: 80°/s |
| Movement Range (Tilt) | From -15° to 90° (auto-flip) |
| Tilt Speed | Configurable, from 0.1°/s to 80°/s  Preset Speed: 80°/s |
| Proportional Zoom | Support |
| Presets | 300 |
| Patrol Scan | 8 patrols, up to 32 presets for each patrol |
| Pattern Scan | 4 pattern scans, record time over 10 minutes for each scan |
| Power-off Memory | Support |
| Park Action | Preset/Pattern Scan/Patrol Scan/Auto Scan/Tilt Scan/Random Scan/Frame Scan/Panorama Scan |
| 3D Positioning | Support |
| PTZ Position Display | Support |
| Preset Freezing | Support |
| Scheduled Task | Preset/Pattern Scan/Patrol Scan/Auto Scan/Tilt Scan/Random Scan/Frame Scan/Panorama Scan/Dome Reboot/Dome Adjust/Aux Output |
| **Compression Standard** | |
| Video Compression | Main Stream: H.265+/H.265/H.264+/H.264  Sub-stream: H.265/H.264/MJPEG  Third Stream: H.265/H.264/MJPEG |
| H.264 Type | Baseline Profile/Main Profile/High Profile |
| H.264+ | Support |
| H.265 Type | Baseline Profile/Main Profile/High Profile |
| H.265+ | Support |
| Video Bitrate | 32 Kbps to 16384 Kbps |
| Audio Compression | G.711alaw/G.711ulaw/G.722.1/G.726/MP2L2/PCM |
| Audio Bitrate | G.711alaw/G.711ulaw: 64 Kbps  G.722.1/G.726: 16 Kbps  MP212/PCM: 32 Kbps/64 Kbps/128 Kbps |
| SVC | Support |
| **Smart Features** | |
| Basic Event | Motion Detection, Video Tampering Detection, Exception |
| Smart Event | Intrusion Detection, Line Crossing Detection, Region Entrance Detection, Region Exiting Detection, Object Removal Detection, Unattended Baggage Detection |
| Smart Record | ANR (Automatic Network Replenishment), Dual-VCA |
| ROI | Main stream, sub-stream, and third stream respectively support four fixed areas. |
| **Image** | |
| Max. Resolution | 1920 × 1080 |
| Main Stream | 50Hz: 25fps (1920 × 1080, 1280 × 960, 1280 × 720)  50fps (1280 × 960, 1280 × 720)  60Hz: 30fps (1920 × 1080, 1280 × 960, 1280 × 720)  60fps (1280 × 960, 1280 × 720) |
| Sub-Stream | 50Hz: 25fps (704 × 576, 640 × 480, 352 × 288)  60Hz: 30fps (704 × 480, 640 × 480, 352 × 240) |
| Third Stream | 50Hz: 25fps (1920 × 1080, 1280 × 960, 1280 × 720, 704 × 576, 640 × 480, 352 × 288)  60Hz: 30fps (1920 × 1080, 1280 × 960, 1280 × 720, 704 × 480, 640 × 480, 352 × 240) |
| Image Enhancement | HLC/BLC/3D DNR/Defog/EIS/Regional Exposure/Regional Focus |
| **Network** | |
| Network Storage | Built-in memory card slot, support Micro SD/SDHC/SDXC, up to 256 GB; NAS (NPS, SMB/ CIPS), ANR |
| Protocols | IPv4/IPv6, HTTP, HTTPS, 802.1x, Qos, FTP, SMTP, UPnP, SNMP, DNS, DDNS, NTP, RTSP, RTCP, RTP, TCP/IP, UDP, IGMP, ICMP, DHCP, PPPoE, Bonjour |
| API | Open-ended, support ONVIF, ISAPI, support SDK and Third-Party Management Platform |
| Simultaneous Live View | Up to 20 channels |
| User/Host | Up to 32 users  3 levels: Administrator, Operator and User |
| Security Measures | User authentication (ID and PW), Host authentication (MAC address); HTTPS encryption; IEEE 802.1x port-based network access control; IP address filtering |
| Client | CMS, Guarding Vision |
| Web Browser | IE 8 to 11, Chrome 31.0 to 44, Firefox 30.0 to 51 |
| **Interface** | |
| Audio Interface | 1-ch audio input and 1-ch audio output |
| Network Interface | 1 RJ45 10 M/100 M Ethernet, PoE+ (802.3 at, class4) |
| **General** | |
| Power | 12 VDC and PoE+ (802.3 at, class4)  Max.: 18 W (Max. 7W for IR) |
| Working Temperature | -30°C to 65°C (-22°F to 149°F) |
| Working Humidity | ≤ 90% |
| Protection Level | IP66 Standard, TVS 4000V Lightning Protection, Surge Protection and Voltage Transient Protection |
| Material | ADC 12, PC, PC+10% GF |
| Dimensions | Φ 164.5 mm × 290 mm (Φ 6.48" × 11.42") |
| Weight | Approx. 2 kg (4.41 lb) |

**Available Model**

|  |
| --- |
| NP112-IR/25X |
|  |
| **Dimensions** |



**Accessories**

|  |  |  |
| --- | --- | --- |
|  | 1618ZJ | Wall Mounting Bracket |
|  | 1602ZJ | Wall Mounting Bracket |
|  | 1602ZJ-corner | Corner Mounting Bracket |
|  | 1602ZJ-pole | Vertical Pole Mounting Bracket |
|  | 1602ZJ-box | Wall Mounting Bracket with Junction Box |
|  | 1671ZJ-SDM9 | In-ceiling Mounting Bracket |
| http://www.hikvision.com/uploadfile/image/product/big/20140704153548402.png | 1663ZJ | Ceiling Mounting Bracket |
| http://www.hikvision.com/uploadfile/image/product/big/20121224191322306841.jpg | 1661ZJ | Pendant Mounting Bracket |
| http://www.hikvision.com/uploadfile/image/product/big/20121224191340251082.jpg | 1662ZJ | Pendant Mounting Bracket |
|  | 1619ZJ | Gooseneck Mounting Bracket |
|  | 1100KI | Network Keyboard |
|  | 1005KI | USB Joy-stick |