**IPC**

**Plugin free**

|  |  |
| --- | --- |
| Supported Max. Resolution | ≤3MP (I7 processor is required) |
| Supported Browser | Firefox52 and above，Chrome45 and above |
| Supported Encoding Format | H.264, H.264+, H.265, H.265+ |

**Comparison Chart for Plugin free and Plugin live view**

|  |  |  |  |
| --- | --- | --- | --- |
| Model | Function | Non-Plugin | With Plugin |
| Preview | Preview | Resolution<=3MP  (I7 processor is required) Bitrate<=2M | √ |
| Audio | √ | √ |
| Capture | √ | √ |
| Digital Zoom | √ | √ |
| Window Division | √ | √ |
| Full-Screen | √ | √ |
| Record | √, Only Chrome | √ |
| Audio On | × | √ |
| Playback | Playback | × | √ |
| Download Video | × | √ |
| Picture | Picture | × | √ |
| Application | Application | √ | √ |
| Configuration | Export Device Parameters | √ | √ |
| Import Device Parameters | √ | √ |
| Upgrade | √(Only .dav file format supported) | √ |
| Draw Area | √ | √ |
| Counting | Only support drawing detection line.  OSD display is not supported. | √ |
| Export Log | Support .txt file format | √ |
| Local | × | √ |
| File Path Setting | Only file name can be displayed,  does not show complete path. | √ |

**Revolved Models**

**IP camera**

NC32x V5.5.61 and above

**NVR**

**Plugin free**

|  |  |
| --- | --- |
| Supported Max. Resolution | ≤1080P |
| Supported Browser | Firefox52 and above，Chrome45 and above |
| Supported Encoding Format | H.264, H.265 |

**Comparison Chart for Plugin free and Plugin live view:**

|  |  |  |  |
| --- | --- | --- | --- |
| Model | Function | Non-Plugin | With Plugin |
| Preview | Preview | Resolution≤1080P Bitrate≤2M  POS overlay is not supported.  Fisheye PTZ expansion is not supported. | √ |
| Audio | √ | √ |
| Capture | √ | √ |
| Digital Zoom | √ | √ |
| Window Division | √ | √ |
| Full-Screen | √ | √ |
| Record | √, Only Chrome | √ |
| Audio On | × | √ |
| Playback | Playback | × | √ |
| Synchronous playback | × | √ |
| Transcoded playback | √ | √ |
| Single-frame play | √ | √ |
| Fast forward/ Slow forward | √ | √ |
| Reverse Playback | × | √ |
| Download Video | × | √ |
| Picture | Picture | × | √ |
| Application | Application | √ | √ |
| Configuration | Export Device Parameters | √ | √ |
| Import Device Parameters | √ | √ |
| Upgrade | × | √ |
| Draw Area | √ | √ |
| Export Log | Support .txt file format | √ |
| Local Configuration | × | √ |
| File Path Setting | Only file name can be displayed,  does not show complete path. | √ |

**Revolved Models**

NR51x&NR710&NRA10 NVR with V4.1.50 and above

All 128/256ch Super NVR with V4.1.61 and above

**DVR**

**Plugin free**

|  |  |
| --- | --- |
| Supported Max. Resolution | AR526&ARA26≤1080p  AR324&AR326&AR328&AR524: No limitation |
| Supported Channel | AR526&ARA26: 2ch  AR324&AR326&AR328&AR524: No limitation |
| Supported Browser | Firefox52 and above, Chrome45 and above |
| Supported Encoding Format | H.264, H.264+,H.265,H.265+ |

**Comparison Chart for Plugin free and Plugin live view**

|  |  |  |  |
| --- | --- | --- | --- |
| Model | Function | Non-Plugin | With Plugin |
| Preview | Preview | AR526&ARA26≤1080p  Bitrate≤2M  POS overlay is not supported.  Fisheye PTZ expansion is not supported. | √ |
| Audio | √ | √ |
| Capture | √ | √ |
| Digital Zoom | √ | √ |
| Window Division | √ | √ |
| Full-Screen | √ | √ |
| Record | √, Only Chrome | √ |
| Audio On | × | √ |
| Playback | Playback | √  1ch mainstream+3ch sub streams or 4ch sub streams | √ |
|  | Synchronous playback | × | √ |
|  | Transcoded playback | √ | √ |
|  | Single-frame play | √ | √ |
|  | Fast forward/ Slow forward | √ | √ |
|  | Reverse Playback | × | √ |
|  | Download Video | √ | √ |
| Picture | Picture | √ | √ |
| Application | Application | √ | √ |
| Configuration | Export Device Parameters | √ | √ |
| Import Device Parameters | √ | √ |
| Upgrade | √ | √ |
| Draw Area | √ | √ |
| Export Log | Support .txt file format | √ |
| Local Configuration | × | √ |
| File Path Setting | Only file name can be displayed,  does not show complete path. | √ |