





* **2 Megapixel High Resolution**
* **Analog HD output, up to 1080p resolution**
* **2.8-12mm vari-focal lens**
* **True Day/Night**
* **OSD Menu, 3D DNR, Smart IR**
* **True WDR, up to 120dB**
* **Up to 40m IR distance**
* **Built-in heater(-H)**
* **Up the Coax(Pelco-C protocol)**
* **IP66 weatherproof & vandal-proof**
* **24V AC/ 12V DC**

**Key Features**

**HAC304D-OD4Z**

**HD1080P WDR Motorized VF Vandal Proof IR Dome Camera**

|  |
| --- |
| **Specifications** |
| ***Camera*** |
| Image Sensor | 2MP CMOS Image Sensor |
| Signal System | PAL/NTSC |
| Effective Pixels | 1944(H)\*1092(V) |
| Min. illumination | 0.01 Lux @ (F1.2,AGC ON),0 Lux with IR; 0.014 Lux @ (F1.4,AGC ON),0 Lux with IR |
| Shutter Time | 1/25(1/30)s to 1/50,000s |
| Lens | 2.8-12mm @ F1.4 |
| Lens Mount | φ14 |
| Day & Night | ICR |
| Angle Adjustment | Pan: 0 – 355°, Tilt: 0-75°, Rotation: 0 – 355° |
| Angle of View | 103° - 32.1° |
| CVBS Output | 1Vp-p Composite Output(75/BNC) |
| WDR | 120dB |
| Video Frame Rate | 1080p@25fps/1080p@30fps |
| HD Video Output | 1 Analog HD output |
| S/N Ratio | ＞62dB |
| ***Menu*** |
| Scene | Indoor, Outdoor, Indoor1, LOW-LIGHT |
| Camera ID | On/off (15 characters, position programmable) |
| AGC | Support |
| D/N Mode | Color/BW/SMART |
| White Balance | ATW/AWC-Set/Manual |
| BLC | Support |
| Functions | HSBLC, Digital noise reduction, Digital zoom(62x), Slow shutter, Mirror, Defog, Defect pixel correction, SMART D-ZOOM |
| Anti-flicker | On/Off |
| Privacy Mask | On/Off, maximum 8 zones |
| Motion Detection | On/Off, maximum 4 zones |
| Language | English, Japanese, CHN1, CHN2, Korean, German, French, Italian, Spanish, Polish, Russian, Portuguese, Dutch, Turkish, Hebrew and Arabic |
| ***General*** |
| Operating Conditions | -30 °C – 60 °C (-22 °F – 140 °F), Humidity 90% or less (non-condensing) -H:-40 °C - 60 °C (-40 °F - 140 °F), Humidity 90% or less (non-condensing) |
| Power Supply | 12 VDC±15%; -A: 12 VDC±15% 24 VAC±15%, Heater is available with 24VAC only |
| Power Consumption | Max. 6W; -H: Max. 12W |
| Protection Level | IP66, IK10 |
| IR Range | Up to 40m |
| Heater | Optional |
| Communication | Up the coax, Protocol: Pelco-C(CVBS Output), Perfect View (TVI-Output) |
| Dimensions | Φ 145.3 × 124.2 mm (Φ 5.72” × 4.89”) |
| Weight | 1350 g |
|  |  |





