**HAC334-OD**

**2 MP Ultra-Low Light Dome Camera**



|  |
| --- |
| icon-08 E:\Working Folder\work\work\前端\icon red\icon red\icon\icon-34.png Progressive Scan OSD |
| Smart IR E:\mission\Spec 模板&Icons\icon 新\icon 新\ICR.png E:\Working Folder\work\work\前端\icon red\icon red\icon\Ture WDR.png |

|  |
| --- |
| **Key Features*** 2.0 megapixel high-performance CMOS
* Ultra-Low Light
* 1920x1080 resolution
* 2.8 mm, 3.6 mm, 6 mm fixed focal lens
* 120 dB true WDR, 3D DNR
* EXIR 2.0, Smart IR, up to 20 m IR distance
* IP67, IK10
* Up the Coax
 |

|  |
| --- |
| ***Camera*** |
| Image Sensor | 2.0 megapixel progressive scan CMOS |
| Signal System | PAL/NTSC |
| Frame Rate | PAL: 1080p@25fpsNTSC: 1080p@30fps |
| Resolution | 1920 (H) × 1080 (V) |
| Min. illumination | Color: 0.005 Lux @ (F1.2, AGC ON), 0 Lux with IR |
| Shutter Time | PAL: 1/25 s to 1/50, 000 sNTSC: 1/30 s to 1/50, 000 s |
| Slow Shutter | Max.: 16 times |
| Lens | 2.8 mm, 3.6 mm, 6 mm fixed focal lens |
| Horizontal Field of View  | 103.5° (2.8 mm), 82.6° (3.6 mm), 54.4° (6 mm) |
| Lens Mount | M12 |
| Day & Night | IR cut filter |
| Angle Adjustment | Pan: 0° to 360°, Tilt:0° to 75°, Rotate: 0° to 360° |
| Synchronization | Internal synchronization |
| WDR (Wide Dynamic Range) | > 120 dB |
| ***Menu*** |
| AGC | Support |
| Day/Night Mode | Auto/Color/BW (Black and White) |
| White Balance | ATW/MANUAL |
| Privacy Mask  | ON/OFF, 4 programmable privacy masks |
| Motion Detection | 4 programmable motion areas |
| Backlight Compensation | WDR/BLC /OFF |
| 3D DNR (Digital Noise Reduction) | Level 1 to 10  |
| Language | English, Chinese |
| Functions | Brightness, Sharpness, Mirror, Smart IR  |
| ***Interface*** |
| Video Output | 1 HD analog output |
| ***General*** |
| Operating Conditions | -40 °C to 60 °C (-40 °F to 140 °F), humidity: 90% or less (non-condensation) |
| Power Supply | 12 VDC±25% |
| Power Consumption | Max. 3.2 W |
| Protection Level | IP67, IK10 |
| Material | Metal |
| IR Range | Up to 20 m |
| Communication | Up the coax, Protocol: (TVI output) |
| Dimensions | Φ 111 mm × 82.4 mm (Φ 4.4" × 3.2") |
| Weight | Approx. 350 g (0.77 lb.) |

**Specification**

|  |
| --- |
| **Order Models** |
| HAC334-OD |
| **Dimension** |



|  |
| --- |
| **Accessory** |
| 未标题-2.png1259ZJ Inclined Ceiling Mounting Bracket | untitled1271ZJ-110 Pendant Mounting Bracket  | 1272ZJ-110B Wall Mounting Bracket | 1275ZJ Vertical Pole Mounting Bracket |
| 1280ZJ-DM18Junction Box | 未标题-1.png1258ZJ Wall Mounting Bracket | 1H18Video Balun |  |

20161122\_Draft