**HAC334D-OD4Z**

**2 MP Ultra Low-Light VF Dome Camera**



|  |
| --- |
| icon-08 Motorized VF Lens Progressive Scan OSD |
| Smart IR E:\mission\Spec 模板&Icons\icon 新\icon 新\ICR.png E:\mission\Spec 模板&Icons\icon 新\icon 新\3-Axis.png |

|  |
| --- |
| **Key Features*** 2.0 megapixel high-performance CMOS
* Ultra-Low Light
* 1920x1080 resolution
* Auto focus, 2.8 mm to 12 mm motorized vari-focal lens
* 120 dB true WDR, 3D DNR
* EXIR 2.0, Smart IR, up to 40 m IR distance
* IP67, IK10
* Up the Coax (UTC-C)
 |

|  |
| --- |
| ***Camera*** |
| Image Sensor | 2.0 megapixel progressive scan CMOS |
| Signal System | PAL/NTSC |
| Frame Rate | PAL: 1080p@25fpsNTSC: 1080p@30fps |
| Resolution | 1920 (H) × 1080 (V) |
| Min. illumination | Color: 0.005 Lux @ (F1.2, AGC ON), 0 Lux with IR |
| Shutter Time | PAL: 1/25 s to 1/50, 000 sNTSC: 1/30 s to 1/50, 000 s |
| Slow Shutter | Max. 16 times |
| Lens | 2.8 mm to 12 mm motorized vari-focal lens |
| Horizontal Field of View  | 32.1° to 103° |
| Lens Mount | Φ14 |
| Day & Night | IR cut filter |
| Angle Adjustment | Pan: 0° to 340°, Tilt:0° to 75°, Rotate: 0° to 355° |
| Synchronization | Internal synchronization |
| WDR (Wide Dynamic Range) | > 120 dB |
| ***Menu*** |
| AGC | Support |
| Day/Night Mode | Auto/Color/BW (Black and White) |
| White Balance | ATW/MANUAL |
| Privacy Mask  | ON/OFF, 4 programmable privacy masks |
| Motion Detection | 4 programmable motion areas |
| Backlight Compensation | WDR/BLC /OFF |
| 3D DNR (Digital Noise Reduction) | Level 1 to 10 |
| Language | English, Chinese |
| Functions | Brightness, Sharpness, Mirror, Smart IR  |
| ***Interface*** |
| Video Output | 1 HD analog output |
| ***General*** |
| Operating Conditions | -40 °C to 60 °C (-40 °F to 140 °F), humidity: 90% or less (non-condensation) |
| Power Supply | 12 VDC±25%-A: 12 VDC±25%, 24 VDC±25% |
| Power Consumption | Max. 5.5W-A: Max. 7 W |
| Protection Level | IP67, IK10 |
| Material | Metal |
| IR Range | Up to 40 m |
| Communication | Up the coax, Protocol: UTC-C (TVI output) |
| Dimensions | Φ 145.2 mm × 124.1 mm (Φ 5.72" × 4.89" ) |
| Weight | Approx. 1600 g (3.53 lb.) |

**Specification**

|  |
| --- |
| **Order Models** |
| HAC334D-OD4Z |
| **Dimension** |



|  |
| --- |
| **Accessory** |
| 1273ZJ-140Wall Mounting Bracket | 1275ZJ Vertical Pole Mounting Bracket | 1276ZJCorner Mounting Bracket | untitled1271ZJ-140Pendant Mounting Bracket |
| 1273ZJ-140BWall Mounting Bracket  | 1241ZJ In-ceiling Mounting Bracket  | 1240ZJ Inclined Ceiling Mounting Bracket |  |

**010000170504**

20161122\_Draft