**HAC348D-OD4Z**

**4K Ultra-Low Light Dome Camera**



|  |
| --- |
| icon-08 E:\Working Folder\work\work\前端\icon red\模拟专用图标red\Ultra-Low Light.pngE:\Working Folder\work\work\前端\icon red\模拟专用图标red\Ture WDR.png Smart IR  |
| E:\Working Folder\work\work\前端\icon red\模拟专用图标red\3-axis Adjustment.png E:\Working Folder\work\work\前端\icon red\icon red\icon\icon-34.png |

|  |
| --- |
| **Key Features*** 8.29 MP high performance CMOS
* Ultra-low light
* 3840 × 2160 resolution
* 2.8 – 12mm motorized vari-focal lens
* 120 dB true WDR, 3D DNR
* EXIR 2.0, smart IR, up to 40 m IR distance
* IP67, IK10
* Up the coax (UTC-C)
 |

|  |
| --- |
| ***Camera*** |
| Image Sensor | 8.29 megapixel progressive scan CMOS |
| Signal System | PAL/NTSC |
| Frame Rate | PAL: 8 MP@12.5fps, 5 MP@20fps, 4 MP@25fps, 1080p@25fpsNTSC: 8 MP@15fps, 5 MP@20fps, 4 MP@30fps, 1080p@30fps |
| Resolution | 3840 (H) × 2160 (V) |
| Min. illumination | Color: 0.003 Lux@(F1.2, AGC ON), 0 Lux with IR |
| Shutter Time | PAL: 1/12.5 s to 1/10,000 s NTSC: 1/15 s to 1/10,000 s |
| Slow Shutter | Max. 16 times |
| Lens | 2.8-12mm motorized vari-focal lens |
| Horizontal Field of View  | 102.2° (2.8 mm), 79° (3.6 mm), 50.8° (6 mm) |
| Lens Mount | M12 |
| Day & Night | IR cut filter |
| Angle Adjustment | Pan: 0° to 355°, Tilt:0° to 75°, Rotate: 0° to 355° |
| Synchronization | Internal synchronization |
| WDR (Wide Dynamic Range) | 120 dB |
| ***Menu*** |
| AGC | Support |
| Day/Night Mode | Auto/Color/BW (Black and White) |
| White Balance | Auto/Manual/Natural |
| Privacy Mask  | ON/OFF, 4 programmable privacy masks |
| BLC (Backlight Compensation) | Support |
| 3D DNR (Digital Noise Reduction) | Level 1 to 10 |
| Language | English |
| Functions | Contrast, Sharpness, Saturation, Mirror, Defog, HLC |
| ***Interface*** |
| TVI Video Output | 1 HD analog output |
| CVBS Video Output | 1 CVBS output (75Ω/BNC) |
| ***General*** |
| Operating Conditions | -40 °C to 60 °C (-40 °F to 140 °F), humidity: 90% or less (non-condensation) |
| Power Supply | 12 VDC ±25% |
| Power Consumption | Max. 4.8 W |
| Protection Level | IP67, IK10 |
| Material | Metal |
| IR Range | Up to 40 m |
| Communication | Up the coax, Protocol: UTC-C (TVI output) |
| Dimensions | Ø 111 mm × 82.4 mm (Ø 4.4" × 3.2" ) |
| Weight | Approx. 450 g (0.99 lb.) |

**Specification**

|  |
| --- |
| **Order Models** |
| HAC348D-OD4Z |
| **Dimension** |
|  |
|  |

|  |
| --- |
| **Accessory** |
| 未标题-2.png1259ZJ Inclined Ceiling Mount | untitled1271ZJ-110 Pendant Mount  | 1272ZJ-110B Wall Mount | E:\Working Folder\work\work\2018年\201801\H0T 变焦\支架安装示意图\半球45支架高清图\302701533 DS-1275ZJ-SUS_副本.jpg1275ZJ-SUS Vertical pole mount |
| 1280ZJ-DM18Junction Box | 未标题-1.png1258ZJ Wall Mount | 1H18Video Balun |  |

20161122\_Draft