LPR Settings

Scheduled Image Settings Auto Switch

Image Adjustment= ALL SET TO 50

Exposure= Iris mode auto

Auto iris level 50

Exposure time 1/200

Gain 25

Focus= Manual

Day/Night Switch= Auto

Sensitivity 4

Filtering Time 5

Smart supplement Light ON

Mode Auto

Backlight Settings=BLC OFF

WDR OFF

White Balance= AWB2

Image Enhancement= Digital Noise Reduction Normal

Noise Reduction Level 50

Defog Mode OFF

EIS OFF

Gray Scale [0-250]

Video Adjustment= Mirror OFF

Rotate OFF

Scene Mode Outdoor

Video Standard NTSC(60HZ)

Capture Mode OFF

Number of Lanes 1,

Plate Mode Small,

Country/Region  United States,

Select Mode   Entrance/Exit.