LPR Settings

Scheduled Image Settings Auto Switch

Image Adjustment= ALL SET TO 50

Exposure= Iris mode auto

 Auto iris level 50

 Exposure time 1/200

 Gain 25

Focus= Manual

Day/Night Switch= Auto

 Sensitivity 4

 Filtering Time 5

 Smart supplement Light ON

 Mode Auto

Backlight Settings=BLC OFF

 WDR OFF

White Balance= AWB2

Image Enhancement= Digital Noise Reduction Normal

 Noise Reduction Level 50

 Defog Mode OFF

 EIS OFF

 Gray Scale [0-250]

Video Adjustment= Mirror OFF

 Rotate OFF

 Scene Mode Outdoor

 Video Standard NTSC(60HZ)

Capture Mode OFF

Number of Lanes 1,

Plate Mode Small,

Country/Region  United States,

Select Mode   Entrance/Exit.